**STEINEL Professional Détecteur de présence**

**IR Quattro HD 24m**

**COM1 - encastré blanc**

Dimensions (L x W x H): 70 x 120 x 120 mm; Manufacturer's Warranty: 5 ans; Settings via: Télécommande, Interrupteur DIP, Potentiomètres, Smart Remote; With remote control: Non; Version: COM1 - encastré blanc; PU1, EAN: 4007841002794; Type: Détecteur de présence; Application, place: Intérieur; Application, room: salle de classe, salle de cours, bureau grande surface, entrepôt de stockage haut, zone de production, salle de conférences / salle de réunion, salle du personnel soignant, salle commune, vestiaires, gymnase, réception / hall, parking couvert / garage souterrain; Colour: blanc; Colour, RAL: 9010; Includes corner wall mount: Non; Installation site: plafond; Installation: Encastré, Plafond; IP-rating: IP20; Ambient temperature: de -25 jusqu'à 55 °C; Matière: Matière plastique; Mains power supply: 230 V / 50 – 60 Hz; Fluorescent lamps, electronic ballast: 1500 W; Fluorescent lamps, uncorrected: 1000 VA; Fluorescent lamps, series-corrected: 1000 VA; Fluorescent lamps, parallel-corrected: 1000 VA; Switching output 1, low-voltage halogen lamps: 2000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 300 W; LED lamps > 8 W: 600 W; Capacitive load in μF: 176 µF; Technology, sensors: infrarouge passif, Détecteur de lumière; Mounting height: 2,50 – 10,00 m; Mounting height max.: 10,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Oui; Capability of masking out individual segments: Non; Electronic scalability: Non; Mechanical scalability: Oui; Reach, radial: 8 x 8 m (64 m²); Reach, tangential: 20 x 20 m (400 m²); Reach, presence: 8 x 8 m (64 m²); Switching zones: 4800 zones de commutation; Functions: Mode normal / mode test, Semi-automatique / Automatique, Mode bouton-poussoir / interrupteur, Manuel ON / ON-OFF, Maintien d'un éclairage constant ON-OFF; Twilight setting: 10 – 1000 lx; Time setting: 30 s – 30 min; Basic light level function: Non; Main light adjustable: Non; Twilight setting TEACH: Oui; Constant-lighting control: Non; Interconnection: Oui; Type of interconnection: Maître/maître, Maître/esclave; Interconnection via: Câble; Interconnection, number: max. 10 capteurs; Product category: Détecteur de présence

**Fabricant** Steinel

**Réf.** 002794

**Désignation commande** IR Quattro HD 24m COM1 - encastré blanc

Livrer, monter et régler pour être opérationnel