**STEINEL Professional Luminaire extérieur LED à détection**

**L 690 S**

**PMMA anthracite V2**

Dimensions (L x W x H): 104 x 291 x 303 mm; With lamp: Oui, système d'éclairage LED STEINEL; Manufacturer's Warranty: 5 ans; Settings via: Potentiomètres; With remote control: Non; Version: PMMA anthracite; PU1, EAN: 4007841053000; Application, place: Extérieur; Application, room: extérieur, entrée, tout autour du bâtiment, Cour et allée; Colour: anthracite; includes sheet of self-adhesive numbers: Oui; Installation site: mur; Impact resistance: IK07; IP-rating: IP44; Protection class: II; Ambient temperature: de -20 jusqu'à 50 °C; Housing material: Aluminium; Cover material: Matière plastique opale; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 8,5 W; Mounting height max.: 2,50 m; Slave modeselectable: Non; Sneak-by guard: Oui; Capability of masking out individual segments: Oui; Electronic scalability: Non; Mechanical scalability: Non; Reach, radial: r = 1.5 m (7 m²); Reach, tangential: r = 7 m (154 m²); Photo-cell controller: Oui; Cover material: caches enfichables; Luminous flux total product: 700 lm; Measured luminos flux (360°): 700 lm; Total product efficiency: 82 lm/W; Colour temperature: 3000 K; Colour variation LED: SDCM3; Lamp: LED non interchangeable; LED life expectancy (max. °C): 50000 h; Service life LED L70B50 (25°): > 60000; Base: sans; LED cooling system: Contrôle thermique passif; Soft light start: Oui; Continuous light: commutable, 4 h; Functions: 4 réglages des programmes fonctionnels axés sur la pratique sur le module amovible du détecteur; Twilight setting: 2 – 1000 lx; Time setting: 5 s – 15 min; Basic light level function: Oui; Basic light level function time: 10/30 min, toute la nuit; Interconnection: Oui; Basic light level function in per cent: 10 %; Basic light level function percentage, from: 10 %; Basic light level function percentage, up to: 10 %; Interconnection via: Câble; Colour Rendering Index CRI: = 82; Optimum mounting height: 2 m; Detection angle: 360 °; Product category: Luminaire extérieur LED à détection

**Fabricant** Steinel

**Réf.** 053000

**Désignation commande** L 690 S PMMA anthracite

Livrer, monter et régler pour être opérationnel