**STEINEL Professional Lampe solaire**

**XSolar L-S**

**anthracite**

Dimensions (L x W x H): 187 x 189 x 298 mm; With lamp: Oui, système d'éclairage LED STEINEL; With motion detector: Oui; Manufacturer's Warranty: 5 ans; Settings via: Potentiomètres; Version: anthracite; PU1, EAN: 4007841085698; Application, place: Extérieur; Application, room: extérieur, entrée, tout autour du bâtiment, terrasse / balcon, Cour et allée; Colour: anthracite; Installation site: mur; Included extension cable: 6 m; Impact resistance: IK03; IP-rating: IP44; Protection class: III; Ambient temperature: de -20 jusqu'à 40 °C; Housing material: Matière plastique; Cover material: Matière plastique transparente; Power supply, detail: Batterie lithium-phosphate de fer 2500 mAh, solaire, indépend. du réseau; Mounting height max.: 2,00 m; Sneak-by guard: Oui; Capability of masking out individual segments: Non; Reach, radial: r = 2 m (5 m²); Reach, tangential: r = 8 m (78 m²); Photo-cell controller: Oui; Measured luminos flux (360°): 150 lm; Colour temperature: 3000 K; Colour Rendering Index: 80-89; Lamp: LED non interchangeable; LED life expectancy (max. °C): 50000 h; Drop in luminous flux in accordance with LM80: L70B10; LED cooling system: Contrôle thermique passif; Soft light start: Non; Functions: Détecteur de mouvement; Twilight setting: 2 lx; Time setting: 10 s – 1 min; Basic light level function: Oui; Basic light level function time: toute la nuit; Basic light level function in per cent: 3 %; Basic light level function percentage, from: 3 %; Basic light level function percentage, up to: 3 %; Output: 1,2 W; Akku-Ladung: ab - 20°; Akku-Funktion: ab - 20; Detection angle: 140 °; Product category: Lampe solaire

**Fabricant** Steinel

**Réf.** 085698

**Désignation commande** XSolar L-S anthracite

Livrer, monter et régler pour être opérationnel