**STEINEL Professional Luminaire extérieur à détection**

**L 400 S**

**noir**

Dimensions (L x W x H): 250 x 215 x 336 mm; With lamp: Non; Manufacturer's Warranty: 5 ans; Settings via: Potentiomètres; With remote control: Non; Version: noir; PU1, EAN: 4007841611019; Application, place: Extérieur; Application, room: extérieur, entrée, tout autour du bâtiment, terrasse / balcon, Cour et allée; Installation site: mur; Impact resistance: IK03; IP-rating: IP44; Protection class: II; Ambient temperature: de -20 jusqu'à 40 °C; Housing material: Matière plastique; Cover material: Verre transparent; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 60 W; Power consumption: 0,8 W; Mounting height max.: 6,00 m; Slave modeselectable: Non; Sneak-by guard: Oui; Capability of masking out individual segments: Oui; Electronic scalability: Non; Mechanical scalability: Non; Reach, radial: r = 3 m (19 m²); Reach, tangential: r = 12 m (302 m²); Photo-cell controller: Oui; Cover material: caches enfichables; Lamp: Lampe d'usage général; Base: E27; Soft light start: Oui; Continuous light: commutable, 4 h; Twilight setting: 2 – 2000 lx; Time setting: 5 s – 15 min; Basic light level function: Oui; Interconnection: Non; Basic light level function in per cent: 0 – 50 %; Basic light level function percentage, from: 0 %; Basic light level function percentage, up to: 50 %; Optimum mounting height: 2 m; Detection angle: 240 °; Product category: Luminaire extérieur à détection

**Fabricant** Steinel

**Réf.** 611019

**Désignation commande** L 400 S noir

Livrer, monter et régler pour être opérationnel